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 TODAY'S TALK
Fill in: the header and the rescue plan before the talk. Then read each line aloud.
1.	OSHA, 29 CFR 1926.501(b)(13): “Each employee engaged in residential construction activities 6 feet (1.8 m) or more above lower levels shall be protected by guardrail systems, safety net system, or personal fall arrest system …” In plain words: anyone 6 feet or more above a lower level needs fall protection. That is the roof edge and the open deck.
2.	Harness on, lanyard clipped to a rated anchor, before you step on the roof. Check the anchor is screwed to a rafter, not just the decking.
3.	Inspect your harness and lanyard now: webbing cuts, bent hooks, stitching. Tag out anything doubtful.
4.	Ladder: 4 to 1 angle, 3 feet above the edge, tied off, feet on solid ground.
5.	Keep the deck clear. Loose shingles, cords and tools cause slips.
6.	Wet, frost or high wind: stop and tell the lead.
7.	Skylights and holes get a cover or a guardrail before anyone works near them.
8.	If someone falls and hangs, call 911 first, then start the rescue plan: ______________________________________ (fill in before the talk)
 SITE CHECK TODAY
☐ Anchors installed     ☐ Harnesses inspected     ☐ Ladders tied off     ☐ Holes and skylights covered
☐ Weather OK     ☐ First-aid kit on site     ☐ Rescue plan known
 SIGN-IN
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Lead signature 		Date 	
Follow your company's safety program and the OSHA rules that apply to your work. This sheet is a reminder, not a substitute.
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